TYPICAL SPECIFICATIONS
TON CONTAINER STORAGE CRADLE

SPECIFICATION  SECTION 11261 - Chlorination Equipment
Storage Cradle Base shall be of fabricated of ASTM-A36 steel and 2-part epoxy finished to resist corrosion.   Cradles shall accommodate chlorine tanks of approximately 30 inch diameter and 3600 lbs gross weight.  Cradles shall not allow tank to rotate.

Storage Cradles shall have holes in ends to attach to floor with anchor bolts or lag bolts.  

Cradles shall carry a minimum of Five (5) Year Warranty.   “Limited” Warranties shall be considered unacceptable.

Cradles shall be CHLOR-SCALE ®   Model 42SC Trunnion Blocks as manufactured by FORCE FLOW, 2430 Stanwell Drive, Concord, CA 94520 USA (www.forceflow.com), or equal.

Model Number:

		Model		Description
		42SC 		Storage Cradle Set (2 per set).   Holds 1 ton container.

File:   _WEB\SPECS\PCS21LHY   02/03/03
FORCE FLOW 1-800-893-6723
FAX: 925-686-6713        
TRUNNIONS